# Transparency Tables for Mode 1

Summary

Transparency Tables for Mode 1 |
Macros |
CPCTM_MASKTABLE0M1 | 256-table (assembly definition) with mask values for mode 1 using pen 0 as transparent
CPCTM_MASKTABLE1M1 | 256-table (assembly definition) with mask values for mode 1 using pen 1 as transparent
CPCTM_MASKTABLE2M1 | 256-table (assembly definition) with mask values for mode 1 using pen 2 as transparent
CPCTM_MASKTABLE3M1 | 256-table (assembly definition) with mask values for mode 1 using pen 3 as transparent

### Macros

### CPCTM_MASKTABLE0M1

256-table (assembly definition) with mask values for mode 1 using pen 0 as transparent

### CPCTM_MASKTABLE1M1

256-table (assembly definition) with mask values for mode 1 using pen 1 as transparent

### CPCTM_MASKTABLE2M1

256-table (assembly definition) with mask values for mode 1 using pen 2 as transparent

### CPCTM_MASKTABLE3M1

256-table (assembly definition) with mask values for mode 1 using pen 3 as transparent

Close