Type Index
$#! · 0-9 · A · B · C · D · E · F · G · H · I · J · K · L · M · N · O · P · Q · R · S · T · U · V · W · X · Y · Z

A |
| Aliases for builtin types
C |
| CPCT_BlendMode
| CPCT_FW_Colour
| CPCT_HW_Colour
| cpct_keyID
F |
| f32
G |
| GLFSR16_TAPSET
I |
| i16
| i32
| i64
| i8
U |
| u16
| u32
| u64
| u8

CPCtelera’s short useful aliases for standard SDCC built-in types.
Enumerates all blending modes for cpct_drawSpriteBlended.
Enumerates all 27 firmware colours
Enumerates all 27 hardware colours
Enumerated type with symbols for all the 80 possible Key/Joy definitions.
float (f32 = float 32-bits, 4 bytes)
This enumeration hold sets of valid TAPS for generating complete pseudo-random sequences using 16-bits Galois LFSR method.
signed int (i16 = integer 16-bits, 2 bytes)
signed long (i32 = integer 32-bits, 4 bytes)
signed long long (i32 = integer 64-bits, 8 bytes)
signed char (i8 = integer 8-bits, 1 byte )
unsigned int (u16 = unsigned 16-bits, 2 bytes)
unsigned long (u32 = unsigned 32-bits, 4 bytes)
unsigned long long (u32 = unsigned 64-bits, 8 bytes)
unsigned char (u8 = unsigned 8-bits, 1 byte )
Close