# Transparency Tables for Mode 0

Summary

Transparency Tables for Mode 0 |
Macros |
CPCTM_MASKTABLE0M0 | 256-table (assembly definition) with mask values for mode 0 using pen 0 as transparent
CPCTM_MASKTABLE1M0 | 256-table (assembly definition) with mask values for mode 0 using pen 1 as transparent
CPCTM_MASKTABLE2M0 | 256-table (assembly definition) with mask values for mode 0 using pen 2 as transparent
CPCTM_MASKTABLE3M0 | 256-table (assembly definition) with mask values for mode 0 using pen 3 as transparent
CPCTM_MASKTABLE4M0 | 256-table (assembly definition) with mask values for mode 0 using pen 4 as transparent
CPCTM_MASKTABLE5M0 | 256-table (assembly definition) with mask values for mode 0 using pen 5 as transparent
CPCTM_MASKTABLE6M0 | 256-table (assembly definition) with mask values for mode 0 using pen 6 as transparent
CPCTM_MASKTABLE7M0 | 256-table (assembly definition) with mask values for mode 0 using pen 7 as transparent
CPCTM_MASKTABLE8M0 | 256-table (assembly definition) with mask values for mode 0 using pen 8 as transparent
CPCTM_MASKTABLE9M0 | 256-table (assembly definition) with mask values for mode 0 using pen 9 as transparent
CPCTM_MASKTABLE10M0 | 256-table (assembly definition) with mask values for mode 0 using pen 10 as transparent
CPCTM_MASKTABLE11M0 | 256-table (assembly definition) with mask values for mode 0 using pen 11 as transparent
CPCTM_MASKTABLE12M0 | 256-table (assembly definition) with mask values for mode 0 using pen 12 as transparent
CPCTM_MASKTABLE13M0 | 256-table (assembly definition) with mask values for mode 0 using pen 13 as transparent
CPCTM_MASKTABLE14M0 | 256-table (assembly definition) with mask values for mode 0 using pen 14 as transparent
CPCTM_MASKTABLE15M0 | 256-table (assembly definition) with mask values for mode 0 using pen 15 as transparent

### Macros

### CPCTM_MASKTABLE0M0

256-table (assembly definition) with mask values for mode 0 using pen 0 as transparent

### CPCTM_MASKTABLE1M0

256-table (assembly definition) with mask values for mode 0 using pen 1 as transparent

### CPCTM_MASKTABLE2M0

256-table (assembly definition) with mask values for mode 0 using pen 2 as transparent

### CPCTM_MASKTABLE3M0

256-table (assembly definition) with mask values for mode 0 using pen 3 as transparent

### CPCTM_MASKTABLE4M0

256-table (assembly definition) with mask values for mode 0 using pen 4 as transparent

### CPCTM_MASKTABLE5M0

256-table (assembly definition) with mask values for mode 0 using pen 5 as transparent

### CPCTM_MASKTABLE6M0

256-table (assembly definition) with mask values for mode 0 using pen 6 as transparent

### CPCTM_MASKTABLE7M0

256-table (assembly definition) with mask values for mode 0 using pen 7 as transparent

### CPCTM_MASKTABLE8M0

256-table (assembly definition) with mask values for mode 0 using pen 8 as transparent

### CPCTM_MASKTABLE9M0

256-table (assembly definition) with mask values for mode 0 using pen 9 as transparent

### CPCTM_MASKTABLE10M0

256-table (assembly definition) with mask values for mode 0 using pen 10 as transparent

### CPCTM_MASKTABLE11M0

256-table (assembly definition) with mask values for mode 0 using pen 11 as transparent

### CPCTM_MASKTABLE12M0

256-table (assembly definition) with mask values for mode 0 using pen 12 as transparent

### CPCTM_MASKTABLE13M0

256-table (assembly definition) with mask values for mode 0 using pen 13 as transparent

### CPCTM_MASKTABLE14M0

256-table (assembly definition) with mask values for mode 0 using pen 14 as transparent

### CPCTM_MASKTABLE15M0

256-table (assembly definition) with mask values for mode 0 using pen 15 as transparent

Close