### bl

List breakpoints. This command prints out information about every fetch and then event breakpoints.

    > bl
    F 1(1) 000160 c2 CLR   P1.0
    D 2(2) 000180 02 LJMP  022a
    F 1(1) 000006 wi
    >

First character on the list shows permanency of the breakpoint. F means fix and D means dynamic. Second item on the list is the hit number associated to breakpoint. After that between the parentheses there is the actual value of the hit counter. If hit counter reaches zero, breakpoint is activated and hit counter is preset with value of hit number. Next item is the address. Next items are different for fetch and event breakpoints.

Fetch breakpoints list hexadecimal code of instruction at breakpoint's address and then disassembled instruction.

Event breakpoints list identification of the event's type.