document.write("\
<P>The different formats are recognised by their sector numbers.  The\
   standard formats for drive A use the same sector numbers as normal.  The\
   first sector numbers of the different formats are:\
<BR><BR><CENTER><TABLE BORDER=1>\
  <TR><TH VALIGN=TOP ROWSPAN=5><B>Drive A</B></TH>\
      <TH>PCW</TH><TD>&amp;01</TD></TR>\
  <TR><TH>Buffer</TH><TD>&amp;11</TD></TR>\
  <TR><TH>System</TH><TD>&amp;41</TD></TR>\
  <TR><TH>Data</TH><TD>&amp;C1</TD></TR>\
  <TR><TH>Other</TH><TD>&amp;81</TD></TR>\
  <TR><TH VALIGN=TOP ROWSPAN=7><B>Drive B</B></TH>\
	  <TH>D1</TH><TD>&amp;01</TD></TR>\
  <TR><TH>D10</TH><TD>&amp;11</TD></TR>\
  <TR><TH>D2</TH><TD>&amp;21</TD></TR>\
  <TR><TH>D20</TH><TD>&amp;31</TD></TR>\
  <TR><TH>D40</TH><TD>&amp;51</TD></TR>\
  <TR><TH>D80</TH><TD>&amp;71</TD></TR>\
  <TR><TH>O</TH><TD>&amp;81</TD></TR>\
</TABLE></CENTER>\
");