document.write("\
<H4>RAMDOS with Basic or Binary programs:</H4>\
<P>Switch on Drive B, THEN switch on the computer and type:\
<BR><P CLASS=code>RUN \"RAMDOS\" <I>ENTER</I></P>\
<P>RAMDOS prompts you state the computer you are using and loads RAMDOS.BIN\
   accordingly.  If the computer is an unexpanded 464 or 664, HIMEM is\
   lowered by about 2K, but if it has the extra 64K of memory, HIMEM is not\
   changed.  Discs for drive B can be formatted using FORMATS (see below).\
<P>The disc commands and BIOS calls work as normal with RAMDOS (ie SAVE,\
   LOAD, |ERA, |REN, |TAPE, |DISC, CALL &amp;BC77 etc etc).\
");