document.write("\
<H4>RAMDOS with CP/M +</H4>\
<P>Put any disc in drive B, and type:\
<P CLASS=code>|CPM</P>\
<P CLASS=code>Type RAMDOS+ D20</P>\
<P>If a disc is not in drive B when CP/M + is loaded, then drive B will\
   not be logged in.\
<P>The discs for drive B can be formatted by using FORMATS (see above).\
   DISCKIT3 cannot be used to format a double sided 80 track disc.  The\
   standard formats (D1, D10, D2, D20, D40, D80) can be called directly by\
   typing\
<P><CODE STYLE='font: 10pt \"Courier New\", Courier;'>RAMDOS+ D10</CODE> or\
   <CODE STYLE='font: 10pt \"Courier New\", Courier;'>RAMDOS+ D2</CODE> etc.\
<P>If RAMDOS+ is entered without a format, you will be prompted for one of these formats\
   or for \"Other\" formats.  The \"Other\" option enables you to change the Disc\
   Parameter Blocks directly.\
");