# Aliases for builtin types

CPCtelera’s short useful aliases for standard SDCC built-in types.

u8 | unsigned char (u8 = unsigned 8-bits, 1 byte )
i8 | signed char (i8 = integer 8-bits, 1 byte )
u16 | unsigned int (u16 = unsigned 16-bits, 2 bytes)
i16 | signed int (i16 = integer 16-bits, 2 bytes)
u32 | unsigned long (u32 = unsigned 32-bits, 4 bytes)
i32 | signed long (i32 = integer 32-bits, 4 bytes)
u64 | unsigned long long (u32 = unsigned 64-bits, 8 bytes)
i64 | signed long long (i32 = integer 64-bits, 8 bytes)
f32 | float (f32 = float 32-bits, 4 bytes)

Close